Laboratory work #9

Frequency response

***Task 1:*** Generate a signal, add some Gaussian noise, and remove noise with the help of commands such as fft, and ifft.

***Task 2:*** Create an input signal x(t) and plot its frequency spectrum. Obtain from the different equation of a filter, the filter’s impulse response h(t), frequency response H(f), and plot it.